
Lab-Network Configuration:  
1- show all connections



2- display all config setting for the active connection

Text

Description automatically generated  
3- show device status

Text

Description automatically generated  
4- display the setting of the eno16777736 interface

Text


Description automatically generated  
5- create a static connection with the same IP address, network, prefix and default gateway.  
Name the new connection static-eth0 with ip 172.25.0.11,netmask 255.255.255.0 and  
gateway 172.25.0.254

Graphical user interface, text

Description automatically generated

6- modify the new connection to add DNS

  
7- activate the new connection

  
8- view the active connection


Text


Description automatically generated  
9- verify the ip address using ip command

  
10- verify the default gateway

Text

Description automatically generated  
11- ping the DNS






12- disable the original connection autostarting at boot

  
13- reboot the system

Reboot

14- view the active connections

­

17- display the current host name

A picture containing graphical user interface

Description automatically generated  
18- display the host name status

Text

Description automatically generated

19- change the hostname and hostname config file  


20- verify the configuration file providing the hostname at network start

Text

Description automatically generated